Customize Device Boot-up First Frame

## Applicable Products

Goblin; Pico Neo; G2

## Instructions Of Removing Existing First Frame

System version requirements: Goblin-b175, pico neo-b133; (Implemented in PUI version 2.3.0)

Modification Scheme: Execute four ADB commands by following the procedure

1. adb reboot bootloader

After executing the first line of command, wait for half a minute and device will enter Root Mode;

1. fastboot oem splash unlock
2. fastboot flash splash XXX.img

Get splash.img file path:<https://github.com/picoxr/support/blob/master/Assets/splash.img>

1. fastboot reboot
2. Reboot device. Check if the first frame Logo has been removed.

## Instructions Of Updating Customized First Frame

* + 1. Provide an image of 280\*280 pixel in PNG format (No black colour involved in the image; No rasterized image or vector image);
    2. Release a new ROM version;
    3. Update custom ROM offline via SD card (See 12.2 for UpdateMethod)