Method to catch log

## Applicable products

Pico Goblin, Pico Neo; Pico Goblin 2;

## Steps

1. Hold “confirm and volume -” to enter 2D settings interface
2. Enter “About Device” - tap PUI version 8 times - return
3. Developer Options - slide down - log settings
4. log toggle - enabled (log storage location - internal storage)
5. Reboot Goblin
6. Reproduce problems
7. Connect Goblin to computer
8. Internal storage devices - logcatch - copy kerne and logcat.log. Which means catch logo.